inq
Prev | Orchestra Opcodes and Operators | Next

## inq

inq — Reads quad audio data from an external device or stream.

## Description

Reads quad audio data from an external device or stream.

| Warning
This opcode is designed to be used only with orchestras that have nchnls_i=4. Doing so with orchestras with nchnls_i > 4 will cause incorrect audio input.

## Syntax

    ar1, ar2,  ar3, a4 inq

## Performance

Reads quad audio data from an external device or stream. If the command-line -i flag is set, sound is read continuously from the audio input stream (e.g. stdin or a soundfile) into an internal buffer. Any number of these opcodes can read freely from this buffer.

## Examples

Here is an example of the inq opcode. It uses the file inq.csd.

Example 458. Example of the inq opcode.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    -odac  -idac ;;;realtime audio I/O
    ; For Non-realtime ouput leave only the line below:
    ; inq.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    sr   = 44100
    ksmps   = 32
    nchnls   = 2	;2 channels out
    0dbfs    = 1
    nchnls_i = 4	;4 channels in

    instr 1 ;4 channels in, two channels out

    ain1, ain2, ain3, ain4 inq		;grab your mics and sing

    adel   linseg 0, p3*.5, 0.02, p3*.5, 0	  ;max delay time = 20ms
    adel2  linseg 0.02, p3*.5, 0, p3*.5, 0.02 ;max delay time = 20ms
    aoutl  flanger ain1, adel, .7
    aoutr  flanger ain2, adel*2, .8
    aoutla flanger ain3, adel2, .9
    aoutra flanger ain4, adel2*2, .5
    ;write to quad file, 16 bits with header
           fout "in_4.wav", 14, aoutl, aoutr, aoutla, aoutra
           outs (aoutl+aoutla)*.5, (aoutr+aoutra)*.5 ;stereo out

    endin
    </CsInstruments>
    <CsScore>

    i 1 0 10
    e
    </CsScore>
    </CsoundSynthesizer>

## See Also

diskin, in, inh, inh, ino, ins, soundin

## Credits

Authors: Barry L. Vercoe, Matt Ingalls/Mike Berry
MIT, Mills College
1993-1997

Prev | Up | Next
ino | Home | inrg