ctrlinit
Prev | Orchestra Opcodes and Operators | Next

## ctrlinit

ctrlinit — Sets the initial values for a set of MIDI controllers.

## Description

Sets the initial values for a set of MIDI controllers.

## Syntax

    ctrlinit ichnl, ictlno1, ival1 [, ictlno2] [, ival2] [, ictlno3] \
          [, ival3] [,...ival32]

## Initialization

ichnl -- MIDI channel number (1-16)

ictlno1, ictlno1, etc. -- MIDI controller numbers (0-127)

ival1, ival2, etc. -- initial value for corresponding MIDI controller number, in the range 0 to 127.

| Note
If this opcode is to be used with a scaling opcode such as ctrl7 the ival1.. should be 127*(initial-min)/(max-min)

## Performance

Sets the initial values for a set of MIDI controllers.

## Examples

Here is an example of the ctrlinit opcode. It uses the file ctrlinit.csd.

Example 192. Example of the ctrlinit opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    -d
    </CsOptions>
    <CsInstruments>

    sr = 44100
    nchnls = 1
    0dbfs = 1

    ctrlinit 1,1,64 ; init control to 64.

    instr 1
     kval ctrl7 1,1,0,1  ; read in the range 0-1
     printk2 kval   ; prints 0.50394
    endin

    </CsInstruments>
    <CsScore>
    i1 0 1
    </CsScore>
    </CsoundSynthesizer>

## See Also

massign

## Credits

Author: Barry L. Vercoe - Mike Berry
MIT, Cambridge, Mass.

New in Csound version 3.47

Thanks goes to Rasmus Ekman for pointing out the correct MIDI channel and controller number ranges.

Prev | Up | Next
ctrl7 | Home | cuserrnd