allpole
Prev | Orchestra Opcodes and Operators | Next

## allpole

allpole — Allpole filter implementation using direct convolution.

## Description

This opcode implements an allpole filter using direct convolution.

## Syntax

    ares allpole asig, kCoef[]

## Performance

kCoef[] -- all-pole filter coefficients (iord-size array)

asig -- audio input

ares -- audio output

This opcode is part of a suite of streaming linear prediction opcodes. It implements an allpole filter using coefficients passed to it via a k-rate array. The filter length is determined by the array size

The typical application is compute the coefficients via some method and then pass these to the opcode. The set of coefficients passed to allpole need to implement a stable filter, since this is an IIR filter and stability is not guaranteed by default.

The most common method of coefficient derivation is linear prediction analysis, produced for instance by lpcanal. Other methods may be employed, including direct calculation of coefficients from a known filter recipe (e.g. resonators etc).

## Examples

Here is an example of the allpole opcode using an audio input signal as lpc source. It uses the file allpole.csd.

Example 51. Example of the allpole opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    -odac -d
    </CsOptions>
    <CsInstruments>

    sr = 44100
    ksmps = 64
    nchnls = 1
    0dbfs = 1

    gifw ftgen 0,0,1024,20,2,1

    instr 1
    a1 diskin "fox.wav",1,0,1
    kcfs[],krms,kerr,kcps lpcanal a1,1,128,1024,64,gifw
    if kcps > 180 then
      kcps = 180
    endif
    a2 buzz 0dbfs, kcps, sr/(kcps*2), -1
    a3 allpole a2*krms*kerr,kcfs
    a3 dcblock a3
    out a3
    endin

    </CsInstruments>
    <CsScore>
    i1 0 30
    </CsScore>
    </CsoundSynthesizer>

Here is another example of the allpole opcode, now using a function table as lpc source. It uses the file allpole-2.csd.

Example 52. Another example of the allpole opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    -odac -d
    </CsOptions>
    <CsInstruments>

    sr = 44100
    ksmps = 64
    nchnls = 1
    0dbfs = 1

    gifn ftgen 0,0,0,1,"fox.wav",0,0,1
    gifw ftgen 0,0,1024,20,2,1

    instr 1
    k1 init 0
    kts = p4
    kcfs[],krms,kerr,kcps lpcanal k1,1,gifn,1024,ksmps,gifw
    if kcps > 180 then
      kcps = 180
    endif
    a1 buzz 0dbfs, kcps, sr/(kcps*2), -1
    a3 allpole a1*krms*kerr,kcfs
    k1 += ksmps*kts
    if k1 > ftlen(gifn) then
     k1 = 0
    endif
    a3 dcblock a3
    out a3
    endin

    </CsInstruments>
    <CsScore>
    i1 0 10 1
    i1 10 10 .75
    i1 20 10 1.5
    </CsScore>
    </CsoundSynthesizer>

## See Also

lpcfilter, lpcanal

Prev | Up | Next
aftouch | Home | alpass