passign
Prev | Orchestra Opcodes and Operators | Next

## passign

passign — Assigns a range of p-fields to ivariables.

## Description

Assigns a range of p-fields to ivariables, or i- or k-array.

## Syntax

     ivar1, ... passign [istart][, iend

     iarray passign [istart][, iend

     karray passign [istart][, iend

## Initialisation

The optional argument istart gives the index of the first p-field to assign. The default value is 1, corresponding to the instrument number.

The optional argument iend gives the index of the last p-field to assign. The default value is 0, which means all.

One of the variables can be a string variable, in which case it is assigned the only string parameter, if there is one, or an error otherwise.

## Performance

passign transfers the instrument p-fields to instrument variables, starting with the one identified by the istart argument. There should not be more variables than p-fields, but there may be fewer.

passign can transfer the instrument p-fields to a one dimensional array, either an iarray or a karray.

## See Also

assign, pcount.

## Example

Here is an example of the passign opcode. It uses the file passign.csd.

Example 705. A variant of toot8.csd that uses passign.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    -odac     ;;;realtime audio out
    ;-iadc    ;;;uncomment -iadc if real audio input is needed too
    ; For Non-realtime ouput leave only the line below:
    ; -o passign.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    sr = 44100
    ksmps = 32
    nchnls = 2
    0dbfs  = 1

    instr 8

    idur,iamp,iskiptime,iattack,irelease,irvbtime,irvbgain  passign   3

    kamp      linen     iamp, iattack, idur, irelease
    asig      soundin   "fox.wav", iskiptime
    arampsig  =         kamp * asig
    aeffect   reverb    asig, irvbtime
    arvbretrn =         aeffect * irvbgain
    ;mix dry & wet signals
              outs      arampsig + arvbretrn, arampsig + arvbretrn

              endin

    </CsInstruments>
    <CsScore>

    ;ins strt dur  amp  skip atk  rel       rvbt rvbgain
    i8   0    4    .3   0    .03  .1        1.5  .3
    i8   4    4    .3   1.6  .1   .1        3.1  .7
    i8   8    4    .3   0    .5   .1        2.1  .2
    i8   12   4    .4   0    .01  .1        1.1  .1
    i8   16   4    .5   0.1  .01  .1        0.1  .1

    e
    </CsScore>
    </CsoundSynthesizer>

## Credits

Author: John ffitch
University of Bath, Codemist Ltd.
Bath, UK
December 2009

New in version 5.12; end point and array version after 5.12

Prev | Up | Next
partikkelsync | Home | paulstretch