GEN15
Prev | Score Statements and GEN Routines | Next

## GEN15

GEN15 — Creates two tables of stored polynomial functions.

## Description

This subroutine creates two tables of stored polynomial functions, suitable for use in phase quadrature operations.

## Syntax

    f # time size 15 xint xamp h0 phs0 h1 phs1 h2 phs2 ...

## Initialization

size -- number of points in the table. Must be a power of 2 or a power-of-2 plus 1 (see f statement). The normal value is power-of-2 plus 1.

xint -- provides the left and right values [-xint, +xint] of the x interval over which the polynomial is to be drawn. This subroutine will eventually call GEN03 to draw both functions; this p5 value is therefor expanded to a negative-positive p5, p6 pair before GEN03 is actually called. The normal value is 1.

xamp -- amplitude scaling factor of the sinusoid input that is expected to produce the following spectrum.

h0, h1, h2, ... hn -- relative strength of partials 0 (DC), 1 (fundamental), 2 ... that will result when a sinusoid of amplitude

xamp * int(size/2)/xint

is waveshaped using this function table. These values thus describe a frequency spectrum associated with a particular factor xamp of the input signal.

phs0, phs1, ... -- phase in degrees of desired harmonics h0, h1, ... when the two functions of GEN15 are used with phase quadrature.

| Notes
GEN15 creates two tables of equal size, labeled f # and f # + 1. Table # will contain a Chebyshev function of the first kind, drawn using GEN13 with partial strengths h0cos(phs0), h1cos(phs1), ... Table #+1 will contain a Chebyshev function of the 2nd kind by calling GEN14 with partials h1sin(phs1), h2sin(phs2),... (note the harmonic displacement). The two tables can be used in conjunction in a waveshaping network that exploits phase quadrature. Before version 5.16 there was a bug (pointed out by Menno Knevel and fixed by François Pinot) on the number of pfields transmitted to gen13 and gen14 by gen15. The consequence is that all the csd, or orc and sco files that used gen15 before this bug was fixed, are likely to sound different now.

## Examples

Here is an example of the GEN15 routine. It uses the files gen15.csd.

Example 1243. An example of the GEN15 routine.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    -odac  ;;;realtime audio out
    ;-iadc    ;;;uncomment -iadc if realtime audio input is needed too
    ; For Non-realtime ouput leave only the line below:
    ; -o gen15.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>
    ;example from the Csound Book, page 85
    sr = 44100
    ksmps = 32
    nchnls = 2
    0dbfs  = 1

    instr 1

    idur  = p3
    iamp  = p4
    ifrq  = cpspch(p5)        ;pitch
    iswp1 = p6
    iswp2 = p7
    kswp  line   iswp1, p3, iswp2      ;amplitude sweep values
    acosi oscili kswp*.5, ifrq, 2      ;f2=cosine wave
    asine oscili kswp, ifrq, 1         ;f1=sine wave
    atab1 tablei acosi, 33, 1, .5      ;tables a1 to GEN13
    atab2 tablei acosi, 34, 1, .5      ;tables a1 to GEN14
    knrm1 tablei kswp, 35, 1           ;normalizing f35
    knrm2 tablei kswp, 36, 1           ;normalizing f36
    anrm1 = atab1*knrm1                ;normalize GEN13 signal
    anrm2 = atab2*knrm2*asine          ;normalize GEN14 signal
    amix  = anrm1+anrm2                ;mix GEN13 and GEN14
    kenv  expseg .001, idur*.1, iamp, idur*.1, iamp*.8, idur*.8, .001
    asig  = amix*kenv
          outs   asig, asig

    endin

    </CsInstruments>
    <CsScore>
    f 1 0 8193 10  1        ;sine wave
    f 2 0 8193  9  1 1 90   ;cosine wave

    ; Note that all the f33 tables in the following sections are defined with p4=-15,
    ; which means that tables 33 and 34 will not be normalized. Thus if we display
    ; tables when running this example, we'll get correct diagrams even if one table
    ; has very small values instead of 0 values, due to cpu approximations in processing
    ; sin(180), as in sections 2, 4, and 5. This has no consequence on the audio result,
    ; because of the use of amp normalization (tables 35 and 36).

    f 33 0 8193 -15 1 1 1 0 1 180 .8 45 .6 270 .5 90 .4 225 .2 135 .1 315  ;makes function tables 33 and 34
    f 35 0 4097  4  33 1    ;amp normalization for f33
    f 36 0 4097  4  34 1    ;amp normalization for f34
    i 1 0 5  .6  8.00 0   1
    i 1 + .  .6  8.00 1   0
    s
    ;even harmonics with no phase shift, odd harmonics with phase shift
    f 33 0 8193 -15 1 1 1 0 1 0 1 180 1 180 1 0 1 0 1 180 1 180 1 0 1 0 1 180 1 180
    f 35 0 4097  4  33 1    ;amp normalization for f33
    f 36 0 4097  4  34 1    ;amp normalization for f34
    i 1 0  5 .6  8.00 0   1
    i 1 +  . .6  8.00 1   0
    s
    ;different harmonic strenghts and phases
    f 33 0 8193 -15 1 1 1 0 1 0 .9 180 .5 270 .75 90 .4 45 .2 225 .1 0
    f 35 0 4097  4  33 1    ;amp normalization for f33
    f 36 0 4097  4  34 1    ;amp normalization for f34
    i 1 0 5 .6  8.00 0  1
    i 1 + . .6  8.00 1  0
    s
    ;lower harmonics no phase shift, upper harmonics with phase shift
    f 33 0 8193 -15 1  1  1 0 1 0 .5 0 .9 0 .3 0 .75 0 .2 180 .6 180 .15 180 .5 180 .1 180
    f 35 0 4097  4  33 1    ;amp normalization for f33
    f 36 0 4097  4  34 1    ;amp normalization for f34
    i 1 0 5 .6  8.00 0   1
    i 1 + . .6  8.00 1   0

    s
    ;lower harmonics with phase shift, upper harmonics no phase shift
    f 33 0 8193 -15 1 1 1 180 1 180 .5 180 .9 180 .3 180 .75 180 .2 0 .6 0 .15 0 .5 0 .1 0
    f 35 0 4097 4 33 1    ;amp normalization for f33
    f 36 0 4097 4 34 1    ;amp normalization for f34
    i 1 0 5 .6  8.00 0  1
    i 1 + . .6  8.00 1  0
    e
    </CsScore>
    </CsoundSynthesizer>

These are the diagrams of the waveforms of the GEN15 routine, as used in the example (in each diagram, the curve in blue is for ftable 33 and the curve in green is for table 34):

f 33 0 8193 -15 1 1 1 0 1 180 .8 45 .6 270 .5 90 .4 225 .2 135 .1 315

f 33 0 8193 -15 1 1 1 0 1 0 1 180 1 180 1 0 1 0 1 180 1 180 1 0 1 0 1 180 1 180

f 33 0 8193 -15 1 1 1 0 1 0 .9 180 .5 270 .75 90 .4 45 .2 225 .1 0

f 33 0 8193 -15 1 1 1 0 1 0 .5 0 .9 0 .3 0 .75 0 .2 180 .6 180 .15 180 .5 180 .1 180

f 33 0 8193 -15 1 1 1 180 1 180 .5 180 .9 180 .3 180 .75 180 .2 0 .6 0 .15 0 .5 0 .1 0

## See Also

GEN13, and GEN14.

Prev | Up | Next
GEN14 | Home | GEN16