pan2
Prev | Orchestra Opcodes and Operators | Next

## pan2

pan2 — Distribute an audio signal across two channels.

## Description

Distribute an audio signal across two channels with a choice of methods.

## Syntax

    a1, a2 pan2 asig, xp [, imode]

## Initialization

imode (optional) -- mode of the stereo positioning algorithm. 0 signifies equal power (harmonic) panning, 1 means the square root method, 2 means simple linear and 3 means an alternative equal-power pan (based on an UDO). The default value is 0.

## Performance

pan2 takes an input signal asig and distributes it across two outputs (essentially stereo speakers) according to the control xp which can be k- or a-rate. A zero value for xp indicates hard left, and a 1 is hard right.

## Example

Here is an example of the pan2 opcodes. It uses the file pan2.csd.

Example 694. Example of the pan2 opcodes.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    -odac     ;;;realtime audio out
    ;-iadc    ;;;uncomment -iadc if real audio input is needed too
    ; For Non-realtime ouput leave only the line below:
    ; -o pan2.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    sr = 44100
    ksmps = 32
    nchnls = 2
    0dbfs  = 1

    giSine ftgen 0, 0, 2^10, 10, 1

    instr 1

    kline	line	0, p3, 1     ; straight line
    ain	oscili	.6, 440, giSine ; audio signal..
    aL,aR	pan2	ain, kline   ; sent across image
    	outs	aL, aR

    endin
    </CsInstruments>
    <CsScore>
    i1 0 5
    e
    </CsScore>
    </CsoundSynthesizer>

## Credits

Author: John ffitch
University of Bath, Codemist Ltd.
Bath, UK
September 2007

New in version 5.07

Prev | Up | Next
p | Home | pan