# Chart Formats

### OpenCPN supported chart formats

#### Raster Charts

BSB Versions 1, 2 and 3, with chart files ending with “.kap”. Many of these charts also comes with a text file with the “.bsb” extension, that is not used at all in OpenCPN.
This is the de facto standard format used by the US NOAA, New Zealand and Brazil, just to name a few.

BSB Version 4, with chart files ending with “.cap”
works with a non free plugin, for Windows only. See the PlugIns download page. This format is used for Canadian charts and others.

Nv-charts with chart files ending with “.eap”
are supported through a non free plugin, for Windows only. See the PlugInsdownload page. “nv-charts” are available for many parts of the world.

NOS/GEO Version 1, with chart files ending with “.nos” and “.geo”
Subsequent versions are probably supported but need to be tested. However, this format is obsolete for new charts.

#### Vector Charts

S57 ENC charts, with chart files ending with “.000”.
ENC update files (ending with .001, .002, …) are included automatically, if present, and must be placed in the same directory as the corresponding base chart (.000). OpenCPNs internalSENC files has a “.S57” file extension.

Senc (Proprietary)
If a chart is said to be a S57 Vector chart, and has a different file ending, it is likely to be a SENC file, a processed version of a “.000” chart file, in a proprietary, platform specific format, that OpenCPN can't handle, unless the extension is “.oesenc”.

Inland ENCs
OpenCPN supports the international Inland ENC standard (S57 based).

S63 Encrypted ENC charts, with chart files ending with “.os63”.
This chart format is supported in OpenCPN from version 4. It is the format for all vector charts from national hydrographic offices worldwide. Apart from being encrypted, S63 charts are exactly the same as S57.

All S63 charts worldwide, from O-charts.org are available for purchase.

- The support is through a two part plugin, one part open source and the other part closed. The encryption and the commercial aspect is handled by a separate entity, o-charts.org

CM93 Version 2.
(C-map Version 3, and later, are in a preprocessed proprietary SENC format and are not supported.)

- Read this please: “The first thing to check if using CM93 is the version!!! Of course we read that version 3 could not be used but we didn't verify it to the bitter end. It was our fault. One way to tell what version you have is that V2 has extra chart folders plus extra files which include the .EXD file. V3 does not have the extra files.”
- Read the whole sad story with a happy ending On Cruisers Forum. So use CM93 Version 2
- Check Chart Files tab go to the directory that is listed and have a look at the files you see. If you have the whole world, there should be 144 folders with 8 digit numeric names, and a handful of separate files. If you see less than 144 folders, that's OK. It just means you don't have the whole world. If the folder does not look like that then it is not the standard CM93 format. – If they don't work, verify that they are Version 2.

### Pictures of charts, can be converted, and used.

### Not supported formats that can be converted.

#### WCI charts

The necessary utilities for making or converting charts usually only run on Windows or Linux. For Mac OS X, use boot camp, Parallels or VMware to run one of these operating systems.

#### OziExplorer

Charts consisting of picture in one of the standard formats, together with a georeferencing “.map” file, can be converted to a bsb kapfile. and a more developed windows version Map2kap-Ozi-2- OpenCPNOzi charts of the ozfx2 or ozfx3 format can not be converted with this tool. These Ozi formats are not documented and proprietary, and cannot be displayed in OpenCPN.

#### HDR/PCX Charts

The HDR format is from an era when computer-memory and processing power were less powerful than today, as a consequence these charts are not of the same quality as more modern charts. Furthermore, most of these charts are not using WGS 84 as reference datum. These charts should not be the first choice, but can be useful if nothing else is available.

### Other formats that are not supported.

The Hydrographic Chart Raster Format, HCRF, used by the United Kingdom Hydrographic Offices' ARCS (Admiralty Raster Chart Service). This is also due to proprietary encryption algorithms and copyright issues. UKHO is now alone in using this format, since New Zeeland switched to the BSB/Kap format and Australia no longer publishes official raster charts.

Charts from Mapmedia, Navionics, C-map (with the exception of CM93 version 2), Garmin and various other private vendors, are not supported, for the same reasons as for the other proprietary charts. It is not possible for users to convert these charts to an OpenCPN recognized format, but it is possible for these companies, to release OpenCPN plugins, if they wish.