CONFIG_LOGO_LINUX_CLUT224_FILE="drivers/video/logo/logo_gokrazy_clut224.ppm"

CONFIG_IPV6=y
CONFIG_DYNAMIC_DEBUG=y

# For Squashfs (root file system):
CONFIG_SQUASHFS=y
CONFIG_SQUASHFS_FILE_CACHE=y
CONFIG_SQUASHFS_DECOMP_MULTI_PERCPU=y
CONFIG_SQUASHFS_ZLIB=y
CONFIG_SQUASHFS_FRAGMENT_CACHE_SIZE=3

# For a console on HDMI:
# # TODO: the simpledrm driver just does not work for me. the ASRock logo never disappears from HDMI
# # [    0.364059] [drm] Initialized simpledrm 1.0.0 20200625 for simple-framebuffer.0 on minor 0
# CONFIG_DRM_SIMPLEDRM=y
# CONFIG_X86_SYSFB=y
#
# Whereas with (working) efifb, I see:
# # [    0.460084] efifb: probing for efifb
# # [    0.460096] efifb: framebuffer at 0xe9000000, using 3072k, total 3072k
# # [    0.460099] efifb: mode is 1024x768x32, linelength=4096, pages=1
# # [    0.460101] efifb: scrolling: redraw
# # [    0.460103] efifb: Truecolor: size=8:8:8:8, shift=24:16:8:0
CONFIG_DRM_SIMPLEDRM=n
CONFIG_X86_SYSFB=n
CONFIG_FB=y
CONFIG_FB_EFI=y
CONFIG_FB_SIMPLE=y
CONFIG_DRM_FBDEV_EMULATION=y
CONFIG_FRAMEBUFFER_CONSOLE=y

# For FUSE (for cpu(1)):
CONFIG_FUSE_FS=y

# For using github.com/vishvananda/netlink
CONFIG_NETFILTER_NETLINK_QUEUE=y
CONFIG_XFRM_USER=y

# For nftables:
CONFIG_NF_TABLES=y
CONFIG_NF_NAT_IPV4=y
CONFIG_NF_CONNTRACK=y
CONFIG_NF_NAT=y
CONFIG_NF_NAT_MASQUERADE_IPV4=y
CONFIG_NFT_PAYLOAD=y
CONFIG_NFT_EXTHDR=y
CONFIG_NFT_META=y
CONFIG_NFT_CT=y
CONFIG_NFT_RBTREE=y
CONFIG_NFT_HASH=y
CONFIG_NFT_COUNTER=y
CONFIG_NFT_LOG=y
CONFIG_NFT_LIMIT=y
CONFIG_NFT_NAT=y
CONFIG_NFT_COMPAT=y
CONFIG_NFT_MASQ=y
CONFIG_NFT_MASQ_IPV4=y
CONFIG_NFT_REDIR=y
CONFIG_NFT_REJECT=y
CONFIG_NF_TABLES_IPV4=y
CONFIG_NFT_REJECT_IPV4=y
CONFIG_NFT_CHAIN_ROUTE_IPV4=y
CONFIG_NFT_CHAIN_NAT_IPV4=y
CONFIG_NF_TABLES_IPV6=y
CONFIG_NFT_CHAIN_ROUTE_IPV6=y
CONFIG_NFT_OBJREF=y
CONFIG_NFT_DUP_IPV4=y
CONFIG_NFT_FIB_IPV4=y
CONFIG_NFT_DUP_IPV6=y
CONFIG_NFT_FIB_IPV6=y
CONFIG_NF_DEFRAG_IPV4=y
CONFIG_NF_DEFRAG_IPV6=y
CONFIG_NETFILTER_XTABLES=y

# Explicitly disable nftables helper modules to prevent NAT slipstreaming attacks:
# https://samy.pl/slipstream/
CONFIG_NF_CONNTRACK_AMANDA=n
CONFIG_NF_CONNTRACK_FTP=n
CONFIG_NF_CONNTRACK_H323=n
CONFIG_NF_CONNTRACK_IRC=n
CONFIG_NF_CONNTRACK_NETBIOS_NS=n
CONFIG_NF_CONNTRACK_SNMP=n
CONFIG_NF_CONNTRACK_PPTP=n
CONFIG_NF_CONNTRACK_SANE=n
CONFIG_NF_CONNTRACK_SIP=n
CONFIG_NF_CONNTRACK_TFTP=n

# For using USB mass storage
CONFIG_USB_EHCI_HCD=y
CONFIG_USB_XHCI_HCD=y
CONFIG_USB_DEVICEFS=y
CONFIG_USB_STORAGE=y

# For NVMe storage
CONFIG_NVME_CORE=y
CONFIG_BLK_DEV_NVME=y
CONFIG_NVME_MULTIPATH=y
CONFIG_NVME_HWMON=y
CONFIG_NVME_TARGET_PASSTHRU=y

# For https://www.fs.com/products/75602.html and https://www.fs.com/products/75603.html network cards:
CONFIG_I40E=y

# For Intel E810 series network cards:
CONFIG_ICE=y

# For Broadcom 57414 10/25 Gbit/s network card:
CONFIG_BNXT=y

# For Mellanox ConnectX-4 25 Gbit/s network cards:
CONFIG_MLX5_EN=y
CONFIG_MLX5_CORE=y
CONFIG_MLX5_CORE_EN=y
CONFIG_MLX5_INFINIBAND=n

# For apu2c4 ethernet ports
CONFIG_IGB=y

# For Intel I225 ethernet ports (ASRock B550 Taichi):
CONFIG_IGC=y

# For /proc/config.gz
CONFIG_IKCONFIG=y
CONFIG_IKCONFIG_PROC=y

# For kexec
CONFIG_KEXEC_FILE=y

# For apu2c4 watchdog
CONFIG_SP5100_TCO=y

# For WireGuard
CONFIG_NET_UDP_TUNNEL=y
CONFIG_WIREGUARD=y

# For traffic shaping using tc:
CONFIG_NET_SCH_TBF=y

# For measuring CPU temperature:
CONFIG_SENSORS_K10TEMP=y

# For measuring non-CPU temperature and fan speeds:
CONFIG_SENSORS_NCT6683=y

# For Corsair Commander Pro fan controller:
CONFIG_SENSORS_CORSAIR_CPRO=y

# For iproute2’s ss(8):
CONFIG_INET_DIAG=y

# For macvlan ethernet devices:
CONFIG_MACVLAN=y

# For virtio drivers (for qemu):
CONFIG_VIRTIO_PCI=y
CONFIG_VIRTIO_BALLOON=y
CONFIG_VIRTIO_BLK=y
CONFIG_VIRTIO_NET=y
CONFIG_VIRTIO=y
CONFIG_VIRTIO_RING=y
# For watchdog within qemu:
CONFIG_I6300ESB_WDT=y

# For running KVM-accelerated qemu VMs:
CONFIG_KVM=y
CONFIG_KVM_INTEL=y
CONFIG_KVM_AMD=y
CONFIG_KVM_AMD_SEV=y

# For bridge ethernet devices:
CONFIG_BRIDGE=y

CONFIG_EFIVAR_FS=y

# For Ryzen CPUs:
CONFIG_X86_AMD_PLATFORM_DEVICE=y
CONFIG_CPU_FREQ_DEFAULT_GOV_POWERSAVE=y
CONFIG_CPU_FREQ_GOV_POWERSAVE=y
CONFIG_X86_POWERNOW_K8=y
CONFIG_X86_AMD_FREQ_SENSITIVITY=y

# Include hardware interrupt CPU usage in /proc/stat CPU time reporting:
CONFIG_IRQ_TIME_ACCOUNTING=y

# For tun devices, see https://www.kernel.org/doc/Documentation/networking/tuntap.txt
CONFIG_TUN=y

# For runc:
CONFIG_BPF_SYSCALL=y
CONFIG_CGROUP_FREEZER=y
CONFIG_CGROUP_BPF=y
CONFIG_SOCK_CGROUP_DATA=y
CONFIG_NET_SOCK_MSG=y
# For podman:
CONFIG_OVERLAY_FS=y
CONFIG_BRIDGE=y
CONFIG_VETH=y
CONFIG_NETFILTER_ADVANCED=y
CONFIG_NETFILTER_XT_MATCH_COMMENT=y
CONFIG_IP_NF_NAT=y
CONFIG_IP_NF_TARGET_MASQUERADE=y
CONFIG_IP_NF_IPTABLES=y
CONFIG_IP_NF_FILTER=y
CONFIG_NETFILTER_XT_NAT=y
CONFIG_NETFILTER_XT_TARGET_MASQUERADE=y
CONFIG_NETFILTER_XT_MATCH_ADDRTYPE=y
CONFIG_NETFILTER_XT_MATCH_CONNTRACK=y
CONFIG_NETFILTER_XT_MATCH_MULTIPORT=y
CONFIG_NETFILTER_XT_MARK=y
CONFIG_CGROUP_PIDS=y
CONFIG_NF_TABLES_INET=y
CONFIG_NFT_REJECT_INET=y
CONFIG_NFT_FIB_INET=y
CONFIG_NFT_FIB_IPV4=y
CONFIG_NFT_FIB_IPV6=y

# Enable TCP BBR as default congestion control
CONFIG_TCP_CONG_BBR=y
CONFIG_DEFAULT_BBR=y
CONFIG_DEFAULT_TCP_CONG="bbr"

# Linux 6.1:
# In file included from <command-line>:0:0:
# drivers/gpu/drm/i915/i915_sw_fence_work.c: In function 'dma_fence_work_init':
# drivers/gpu/drm/i915/i915_sw_fence.h:57:20: error: the comparison will always evaluate as 'false' for the address of 'fence_notify' will never be NULL [-Werror=address]
#   BUILD_BUG_ON((fn) == NULL);    \
#                     ^
# ././include/linux/compiler_types.h:337:9: note: in definition of macro '__compiletime_assert'
#    if (!(condition))     \
#          ^~~~~~~~~
# ././include/linux/compiler_types.h:357:2: note: in expansion of macro '_compiletime_assert'
#   _compiletime_assert(condition, msg, __compiletime_assert_, __COUNTER__)
#   ^~~~~~~~~~~~~~~~~~~
# ./include/linux/build_bug.h:39:37: note: in expansion of macro 'compiletime_assert'
#  #define BUILD_BUG_ON_MSG(cond, msg) compiletime_assert(!(cond), msg)
#                                      ^~~~~~~~~~~~~~~~~~
# ./include/linux/build_bug.h:50:2: note: in expansion of macro 'BUILD_BUG_ON_MSG'
#   BUILD_BUG_ON_MSG(condition, "BUILD_BUG_ON failed: " #condition)
#   ^~~~~~~~~~~~~~~~
# drivers/gpu/drm/i915/i915_sw_fence.h:57:2: note: in expansion of macro 'BUILD_BUG_ON'
#   BUILD_BUG_ON((fn) == NULL);    \
#   ^~~~~~~~~~~~
# drivers/gpu/drm/i915/i915_sw_fence_work.c:89:2: note: in expansion of macro 'i915_sw_fence_init'
#   i915_sw_fence_init(&f->chain, fence_notify);
#   ^~~~~~~~~~~~~~~~~~
# cc1: all warnings being treated as errors
# make[5]: *** [drivers/gpu/drm/i915/i915_sw_fence_work.o] Error 1
# make[4]: *** [drivers/gpu/drm/i915] Error 2
# make[3]: *** [drivers/gpu/drm] Error 2
CONFIG_WERROR=n

# Enable zstd compression to stay below 15 MB, which is the size of Extended Memory.
# This is relevant to keep the kernel booting with the minimal MBR loader we use.
CONFIG_KERNEL_ZSTD=y

# For qemu -M microvm quick boots:
CONFIG_VIRTIO_MMIO=y

CONFIG_HW_RANDOM_VIRTIO=y
CONFIG_XEN_VIRTIO=y
CONFIG_VIRTIO_IOMMU=y

CONFIG_IPV6_MULTIPLE_TABLES=y
CONFIG_NF_SOCKET_IPV6=y
CONFIG_NETLINK_DIAG=y
CONFIG_INET_DIAG_DESTROY=y

# More AWS stuff:
CONFIG_ENA_ETHERNET=y
CONFIG_RANDOM_TRUST_CPU=y
CONFIG_RANDOM_TRUST_BOOTLOADER=y

# For older AWS:
CONFIG_XEN=y
CONFIG_XEN_DOM0=y
CONFIG_XEN_PRIVILEGED_GUEST=y
CONFIG_XEN_PVHVM=y

# for easy sandboxing with go-landlock
CONFIG_SECURITY_LANDLOCK=y

# For cellular modems
CONFIG_WWAN=y
CONFIG_USB_NET_CDC_MBIM=y

# For physically connecting the gokrazy bakery:
CONFIG_USB_SERIAL=y
CONFIG_USB_SERIAL_FTDI_SIO=y
CONFIG_USB_SERIAL_CP210X=y
CONFIG_USB_SERIAL_CH341=y
# USB driver for GSM and CDMA modems
CONFIG_USB_SERIAL_OPTION=y

